{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["原紙","重量表 (旧)"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":71,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"原紙","index":0,"n_rows":36,"n_cols":21,"rows_kept":36,"cut":false,"hidden":false,"merged":[[5,1,5,3],[5,4,5,20],[0,18,0,20],[3,1,3,3],[3,4,3,5],[3,6,3,12],[3,13,3,14],[3,15,3,20],[4,1,4,3],[4,4,4,5],[4,6,4,14],[4,15,4,16],[4,17,4,20],[0,6,0,13],[1,1,1,5],[6,1,6,3],[6,10,6,11],[6,12,6,13],[6,17,6,20],[7,1,7,3],[7,4,7,11],[7,12,7,16],[7,17,7,20],[8,1,8,3],[8,4,8,11],[8,12,8,20],[9,1,10,3],[9,4,9,11],[9,12,9,20],[10,4,10,11],[10,12,10,20],[11,2,11,6],[11,12,11,16],[12,2,12,6],[12,12,12,16],[13,2,13,6],[13,12,13,16],[14,2,14,6],[14,12,14,16],[15,2,15,6],[15,12,15,16],[16,2,16,6],[16,12,16,16],[17,2,17,6],[17,12,17,16],[18,2,18,6],[18,12,18,16],[19,2,19,6],[19,12,19,16],[20,2,20,6],[20,12,20,16],[21,2,21,6],[21,12,21,16],[22,2,22,6],[22,12,22,16],[28,12,28,16],[23,2,23,6],[23,12,23,16],[24,2,24,6],[24,12,24,16],[25,2,25,6],[25,12,25,16],[26,2,26,6],[26,12,26,16],[27,2,27,6],[27,12,27,16],[28,2,28,6],[35,20,36,20],[32,2,32,6],[32,12,32,16],[33,1,34,1],[33,2,33,16],[34,2,34,16],[35,1,36,5],[35,6,36,15],[35,16,36,17],[29,2,29,6],[29,12,29,16],[30,2,30,6],[30,12,30,16],[31,2,31,6],[31,12,31,16]]}
[null,null,null,null,null,null,"オ ー ダ ー 表"]
[null,"月/　　　　日"]
[]
[null,"会　社　名",null,null,null,null,null,null,null,null,null,null,null,"ＴＥＬ"]
[null,"現　場　名",null,null,null,null,null,null,null,null,null,null,null,null,null,"担当者"]
[null,"住　　　所",null,null,"〒　　　　　-"]
[null,"積　込　日",null,null,null,null,"／",null,null,null,"夜積み・当配",null,"納入日",null,null,"／",null,"AM・PM　   　："]
[null,"納入方法",null,null,"配　達　・　来　社　・　発　送　・　引　取",null,null,null,null,null,null,null,"運　賃　請　求",null,null,null,null,"可　 ・　 不可"]
[null,"運送店名",null,null,null,null,null,null,null,null,null,null,"発送　・　軽量　・　２ｔ ・ ４ｔ　・ ６ｔ　・　８ｔ"]
[null,"その他指示類",null,null,null,null,null,null,null,null,null,null,"１１ｔ　・　増ｔ　・　トレーラー　・　その他"]
[null,null,null,null,null,null,null,null,null,null,null,null,"ランク・値引率"]
[null,null,"品　名　・　品 番",null,null,null,null,"数　量","重　量","小　計","備考",null,"品　名　・　品　番",null,null,null,null,"数　量","重　量","小　計","備考"]
[null,1,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},{"$f":"IF(ISERROR(I13*H13),\"\",I13*H13)","v":""},null,22,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},{"$f":"IF(ISERROR(S13*R13),\"\",S13*R13)","v":""}]
[null,2,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,23,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,3,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,24,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,4,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,25,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,5,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,26,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,6,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,27,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,7,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,28,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,8,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,29,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,9,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,30,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,10,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,31,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,11,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,32,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,12,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,33,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,13,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,34,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,14,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,35,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,15,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,36,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,16,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,37,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,17,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,38,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,18,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,39,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,19,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,40,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,20,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,41,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,21,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",VLOOKUP(#REF!,#REF!,4,FALSE))","v":{"$error":"#REF!"}},"",null,42,null,null,null,null,null,null,{"$f":"IF(ISBLANK(#REF!),\"\",(VLOOKUP(#REF!,#REF!,4,FALSE)))","v":{"$error":"#REF!"}},""]
[null,"その他",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"担当者","安部"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"営担"]
[null,"出庫指示伝票ＮＯ．",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J13:J33)+SUM(T13:T33)","v":0},null,null,null,"ｋｇ"]

{"sheet":"重量表 (旧)","index":1,"n_rows":99,"n_cols":68,"rows_kept":99,"cut":false,"hidden":true,"merged":[]}
[]
[]
["コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量","コード","品番","品名","重量"]
[1,"A4064","鳥居型建枠",17.2,97,"A151","梁渡（７６２用）",6.1,235,"OA-2306A09","SKバンノー受L09",null,338,null,null,null,471,"PNF-15L","スカイフェンス15",7.6,1054,"CG6-12ｶﾌﾟﾗ","妻側手摺 ｴﾝﾄﾞｽﾄｯﾊﾟｰ",2.5,2036,"60K6.0M","角パイプ６０",24.4,3010,"20ｶﾞﾀ","サポート２尺616-945mm",6,3141,"OKSKJ-6040","ＯＫ壁当てジャッキ",3.3,4049,"1ｶﾞﾀM80H","吊足場片面",0,null,null,null,null,6040,"ｶﾌﾟﾗｰ","ﾌﾞﾗｹｯﾄ先端ｸﾗﾝﾌﾟ",0.39,6263,"ALHTR6","ハッチ布板（アルミ）",null,6356,"ﾊﾟｯｶｰ25","２５φ用パッカー",null,7229,"H150-1.37M","Ｈ型鋼１．３７ｍ",43.16,9000,"SP-10L","キリバリサポート"]
[2,"A4055B","1219建枠 H1700",15.4,98,"A152","梁渡（９１４用）",6.5,236,"OA-2306D09","SKバンンー受C09",null,339,null,null,null,472,"PNF-12L","スカイフェンス12",6.4,1055,"CG800CＫ","妻手摺クランプ式",2.5,2037,"60K6.5M","角パイプ６０",26.4,3011,"15ｶﾞﾀ","サポート１．５尺404-623mm",5,3142,"OKSW-18","荷重受梁",17.399999999999999,4052,"TAC","吊足場クランプ",5,5114,"R3x6NB","ラッセルネット青",5.4,6041,"BKH1306","ブラケット",35,6264,"ﾂﾘｻｹﾞｻﾞｲ","階段枠吊り下げ材",null,6400,"AHG45","ＡＬキャスターゲート",44.5,7230,"H150-1.1M","Ｈ型鋼",34.65,9001,"SP-6L","キリバリサポート",12]
[3,"A405","1219調整枠 Ｈ1524",15.1,99,"A153","梁渡（６１０用）",5.6,237,"OA-2306B09","SKバンノー押え09",null,340,"FBH-305","張出ブラケット３０５",2,473,"PNF-09L","スカイフェンス09",5.0999999999999996,1056,"CG800C","妻手摺クランプ付",2.4,2038,"60K7.0M","角パイプ６０",28.4,3012,"10ｶﾞﾀ","サポート１尺315-445mm",4.5,3143,"OKSW-15","荷重受梁",15.8,null,null,null,null,5115,"R5x5NB","ラッセルネット青",7.5,6042,"BKH1606","ブラケット",60,6265,"LS-1010","斜面ノリダー本体",26,6401,"AHG-C1","ゲートクランプ　１",null,7231,"H150-1.0M","Ｈ型鋼１．０ｍ",31.5,9002,"A728","キャスター",4.8,9446,"GB","ゴムバンド中古"]
[4,"A405L","梯子型建枠",15.8,100,null,null,null,238,"OA-2306C09","SKフレ止め09",null,341,"FBH-24","張出ブラケット４０６",2.2000000000000002,474,"PNF-06L","スカイフェンス06",3.7,1057,"CG800","妻手摺",2.4,2039,"60K7.5M","角パイプ６０",30.5,3016,"E5ｶﾞﾀ","補助サポート（５尺）",5.5,3144,"OKSW-12","荷重受梁",12,4060,"BPﾊﾟﾚｯﾄ","防音パネルパレット",null,5116,"R6x6NB","ラッセルネット青",10.8,6043,"NKB300","伸縮ブラケット230-340mm",3.2,6266,"LSD-9","斜面ノリダー手摺",4,6402,"AHG-C2","ゲートクランプ　２",null,7232,"H150-1.5M","Ｈ型鋼１．５ｍ",47.25,9003,"AX11-14ｶﾞﾀ","ホリービーム",11.3,9447,"ﾊﾟﾚｯﾄM","メタルパレット"]
[5,"A404L","1219調整枠 Ｈ1219",12.9,101,"A1453","隅梁受金具",3.3,239,"OA-2306A06","SKバンノー受L06",null,342,"FBH-50","張出ブラケット６１０",2.9,null,null,null,null,1058,"CG600(C)","妻手摺",2,2040,"60K8.0M","角パイプ６０",32.5,3017,"E4ｶﾞﾀ","補助サポート（４尺）",4.7,3145,"OKSW-9","荷重受梁",10.4,4061,"BP06","防音パネル０６",5.2,5117,"R5x10NB","ラッセルネット青",15,6044,"ｶﾌﾟﾗ-300ﾖｳ","先端クランプ３００用",0.39,6269,"ｼｰﾄﾊﾟｲﾙ　3M","鋼矢板２型　３M",null,6403,"AHG-C3","ゲートクランプ　３",0.7,7233,"H150-2.0M","Ｈ型鋼２．０ｍ",63,9004,"AX14-18ｶﾞﾀ","ホリービーム",12.5,9452,"60K1.2M","角パイプ",4.87]
[6,"A403L","1219調整枠 H914",9.3000000000000007,102,"A1471","方杖（3ｽﾊﾟﾝ～用）",7.3,240,"OA-2306D06","SKバンノー受C06",null,343,"FSB-500","Ｆ伸縮ブラケット５０",3.1,490,"CAF-K6A","アルミ台車6輪",25.7,1059,"CG600C・ＯＳ","妻手摺",2,2045,"100K0.75M","角パイプ100",7.14,3018,"E3ｶﾞﾀ","補助サポート（３尺）",4.8,3146,"OKSR-1708","荷重受梁",28,4062,"BP18","防音パネル1800",9.5,5118,"R8x8NB","ラッセルネット青",19.2,6045,"ＱＢ６２４","クイックボード",8.5,6270,"ｼｰﾄﾊﾟｲﾙ　4M","鋼矢板２型　４M",null,6404,"AHG-45-ｱﾙﾏ","アルミクロスゲート",79,7234,"H150-2.5M","Ｈ型鋼２．５ｍ",null,9005,"AX18-25ｶﾞﾀ","ホリービーム",19,9460,"1.0M　（打）","1.0M打ち込み",2.73]
[7,"A417","1219調整枠 H490",8.9,103,"A1475","方杖（2ｽﾊﾟﾝ用）",5.7,241,"OA-2306B06","SKバンノー押え06",null,344,"FSB-750","Ｆ伸縮ブラケット７５",4.7,null,null,null,null,1060,"CG800C・ＯＳ","妻手摺９１４用",2.4,2046,"100K1.0M","角パイプ100",9.52,3021,"PNC","根がらみクランプ",1.6,3147,"OKS-1108","荷重受梁",21,4063,"BPｺｰﾅｰ","防音パネルコーナー",2.2000000000000002,5119,"R4x7NB","ラッセルネット青（透明）",9.3000000000000007,6046,"ＱＢＣ","クイッククランプ",1.9,6271,"ｼｰﾄﾊﾟｲﾙ　6M","鋼矢板２型　６M",null,6405,"AHG-60-ｱﾙﾏ","アルミクロスゲート",null,7235,"H150-3.0M","Ｈ型鋼３．０ｍ",93.3,9006,"AX25-32ｶﾞﾀ","ホリービーム",23,9461,"1.5M　（打）","1.５M打ち込み",4.0999999999999996]
[8,"A4025L","梯子型建枠",10.3,104,"ｶｼﾞｭｳｳｹﾊﾘ","荷重受梁",21.3,242,"OA-2306C06","SKフレ止め06",null,345,"FSB-1000","Ｆ伸縮ブラケット１０",5.8,500,"JFT-2.25","48.6支柱0225",1.3,1061,"A75","棒ジャッキ",4.0999999999999996,2047,"100K1.5M","角パイプ100",14.3,3022,"ALCH38","アルミ強力サポート",null,3148,"OKEC1","ＯＫ専用クランプ直交",1.1000000000000001,4064,"ﾐﾂﾂﾞﾒｸﾗﾝﾌﾟ","三爪クランプ",0.5,5120,"R7x7NB","ラッセルネット青（橙）",15.5,6049,"AL1750S","アングルブラケット",null,6272,"ｼｰﾄﾊﾟｲﾙ　8M","鋼矢板２型　８M",null,6406,"AXG-27","アルミゲート２．７ｍ",52,null,null,null,null,9007,"AX32-39ｶﾞﾀ","ホリービーム",28,0,0,0]
[9,null,null,null,105,"A149(M)","梁枠４スパン分割式L=7600",56,null,null,null,null,346,"FB-24","Ｆブラケット２４",1.8,503,"JFT-13.5","48.6支柱1350",5,1062,"A752","ジャッキベース",3.3,2048,"100K2.0M","角パイプ100",19.100000000000001,3023,"102.5×48.6","上管用直交",null,3149,"OKEC2","ＯＫ専用クランプ自在",1.1000000000000001,4065,"BP15","防音パネル1500",8.3000000000000007,null,null,null,null,null,null,null,null,null,null,null,null,6407,"AXG-36","アルミゲート３．６ｍ",65,7237,"H150-4.0M","Ｈ型鋼４．０ｍ",124.4,9008,"AX39-46ｶﾞﾀ","ホリービーム",35]
[10,null,null,null,106,"A1453-06","隅梁受金具",2.7,246,"SL35-14","スーパーラダー",null,347,"FB-50","Ｆブラケット５０",3.6,504,"JFT-18","48.6支柱1800",6.1,1063,"A752S","ロングジャッキベース",4.5999999999999996,2049,"100K2.5M","角パイプ100",23.8,3024,"120×48.6","下管用直交",null,3150,"OKSISJJ-125","移動用ジャッキ車輪（Ａ）",null,4066,"1219ﾂﾏｶﾞﾜ","コーナー防音1219",0,null,null,null,null,6050,"AL1750","アングルブラケット",60,null,null,null,null,6408,"AHG-P","ゲート用パネル",10,null,null,null,null,9009,"ｷｬｯﾁｸﾗﾝﾌﾟ","ﾏﾙﾁｷｬｯﾁｸﾗﾝﾌﾟ",1.3]
[11,"A3055A","914建枠 H1700",13.1,107,"A8030","布枠",0,247,"SL35-12","スーパーラダー",null,348,null,null,null,505,"JFT-27","48.6支柱2700",9.3000000000000007,1064,"A752H","大引受ジャッキ",4.5999999999999996,2050,"100K3.0M","角パイプ100",28.6,3026,"MSI120","ミドルサポート上管",19.5,3151,"OKSIS-48","移動用支持材（Ａ）",null,4067,"BP12","防音パネル1200",8.8000000000000007,null,null,null,null,6053,"NREｶﾞﾀM","スタンション（Ｍ）",7.1,6273,"PARAPET","パラペット手摺",8.6999999999999993,6409,"AHG-P1","パネル用セットピン",0,7239,"H150-5.0M","Ｈ型鋼５．０ｍ",null,9010]
[12,"A305","914調整枠 H1524",13,108,"A8040","布枠",13.2,248,"SL24-12","スーパーラダー",null,349,null,null,null,506,"JFT-36","48.6支柱3600",11.8,1065,"A752HS","ロング大引受ジャッキ",6.6,2051,"100K3.5M","角パイプ100",33.299999999999997,3027,"MSI80","ミドルサポート上管",13.1,3152,"ＯＫｽｷﾏｲﾀ８１","ＯＫｽｷﾏｲﾀ８１",6.5,4068,"BP09","防音パネル900",6.9,null,null,null,null,6054,"Hｶﾞﾀ",null,null,6274,"KSYA","ＫＳ傾斜足場",7,6410,"AXG-45","アルミゲート４．５ｍ",79,null,null,null,null,9011]
[13,"A304L","914調整枠 H1219",10,112,"A726","キャスター",4,249,"ﾗﾀﾞｰﾂﾘｶﾅｸﾞ","ラダー吊金具",null,350,"FG-3658","梁枠３６５８",21.6,508,"JFT-4.5HV","支柱0450脱着式",1.9,1066,"A753H","大引受ジャッキ",5.0999999999999996,2052,"100K4.0M","角パイプ100",38.1,3028,"MSI50","ミドルサポート上管",8.9,3153,"ＯＫｽｷﾏｲﾀ１１０","ＯＫｽｷﾏｲﾀ１１０",8.5,4069,"ﾌﾟﾙｺﾑ18","透明養生パネル",11.4,null,null,null,null,6055,"SEPAN","折半支柱",2.5,6276,"AL8MS","アルミ２連梯子８M",24,6411,"AXG-54","アルミゲート５．４ｍ",92,7241,"H150-6.0M","Ｈ型鋼６．０ｍ",189,9012,"ﾏﾙﾁﾊﾟﾚｯﾄ","マルチパレット"]
[14,"A303L","914調整枠 H914",8.5,116,"A728Jｼﾛ","ジャッキキャスター白",7.4,250,"HSH-143","ハンガーステージ梁材",9.1999999999999993,351,"FG-5487","梁枠５４８７",36.200000000000003,509,"JFT-09HV","支柱0900脱着式",3.3,1067,"A753HS","大引受ジャッキ",8.5,2053,"100K4.5M","角パイプ100",42.8,3029,"MSI30","ミドルサポート上管",5.9,3154,"ＯＫｽｷﾏｲﾀ１８０","ＯＫｽｷﾏｲﾀ１８０",12.3,4070,"ﾌﾟﾙｺﾑ09","透明養生パネル",0,5133,"06x2K防音","防音シート０６",4.0999999999999996,6056,"SEPAN-B","折半ベース",9,null,null,null,null,6412,"AXG-63","アルミゲート６．３ｍ",105,7242,"I150-1.1M","Ｈ型鋼150ｘ75",14.94,9013,"R0707N","ラッセルネット"]
[15,"A317","914調整枠 H490",7.5,117,"A726J","ジャッキキャスター",5.69,251,"HSS-143","ハンガーステージ斜材",12.2,352,null,null,null,510,"JFN-02","手摺0200",0.9,1068,"PKB","固定ベース",0.8,2054,"100K5.0M","角パイプ100",47.6,3030,"MSI20","ミドルサポート上管",4.3,3155,"ＯＫ－ＦＳＰＲＫ","ＯＫ用先行手摺金具",null,4071,"1K×2K","防音シート",9.8000000000000007,5134,"09x2K防音","防音シート０９",5.6,6060,"H2ｶﾞﾀ","スタンションＨ２型",6.2,null,null,null,null,6413,"ｶﾀﾋﾞﾗｷｶﾅｸﾞ","アルマゲート片開金具",0.5,7243,"I150-1.37M","Ｈ型鋼150ｘ75",19.18,9014,"SX48","軽量ビーム４８",32.5]
[16,null,null,null,118,"A728J","ジャッキキャスター",7.39,252,"HSW-143","ハンガーステージ手摺枠",9.6999999999999993,353,null,null,null,511,"JFN-03","手摺0305",1.2,1069,"A15","固定ベース",1,2055,"100K5.5M","角パイプ100",52.4,3031,"MSO120","ミドルサポート下管",20,3156,"60.5ﾍﾞｰｽ","ＯＫ固定ﾍﾞｰｽ",0.9,4072,"ﾌﾟﾙｺﾑ12","透明養生パネル",null,5135,"12x2K防音","防音シート１２",7.1,6061,"KSH2034","ハンドレール階段用",15.3,null,null,null,null,null,null,null,null,null,null,null,null,9015]
[17,null,null,null,119,"EJ32","伸縮ジャッキ",1.7,253,"HSRT-1","ハンガー幅木１８Ｆ",9.3000000000000007,354,null,null,null,512,"JFN-06","手摺0610",2,1070,"A15H","大引受金具",2.5,2056,"100K6.0M","角パイプ100",57.1,3032,"MSO80","ミドルサポート下管",14.4,3157,"OKS-PJ752H","OKS大引受ピポット",6,4073,"ﾌﾟﾙｺﾑ15","透明養生パネル",null,5136,"15x2K防音","防音シート１５",8.6,6062,"KPH1118","ハンドレール踊り場用",11.9,null,null,null,null,null,null,null,null,null,null,null,null,9016]
[18,null,null,null,120,"CC42","連結クランプ",0.5,254,"HSRT143","ハンガー幅木143",6.3,355,null,null,null,513,"JFN-09","手摺0914",2.7,1071,"A14P","ピポットジャッキ",4.0999999999999996,2057,"100K6.5M","角パイプ100",61.86,3033,"MSO50","ミドルサポート下管",12.1,3177,"OKC-4","センタートラス４３０",null,null,null,null,null,5137,"1K×2K防音","防音シート",9.8000000000000007,6063,"KPH0005","ハンドレール踊り場用",5.2,6277,"LH-36B","イージークライマー大",4.3,null,null,null,null,null,null,null,null,9017]
[19,null,null,null,121,"L500","アウトリガー控枠",9.1,255,"HSA25","ハンガーステージ手摺柱",2.6,356,null,null,null,514,"JFN-12","手摺1219",3.5,1074,"Uﾍﾞｰｽ","建枠上ベース",0.8,2058,"100K7.0M","角パイプ100",66.599999999999994,3034,"MSO30","ミドルサポート下管",9.4,3178,"OKC-8","センタートラス８３０",null,4080,"SXBP18","採光防音パネル18",10.7,5138,"1.82x2K","防音シート(インチ)",9.8000000000000007,6064,"KPH0812","ハンドレール踊り場用",10.5,6278,"AL3M","アルミ梯子３Ｍ",8,null,null,null,null,null,null,null,null,9018]
[20,"A6117R","簡易枠（ア－チ）",11.8,122,"ﾊﾊﾞｷA-RT1","幅木",4.0999999999999996,null,null,null,null,357,null,null,null,515,"JFN-15","手摺1524",4.3,1076,"PJ12","ピポットジャッキ",3.6,2059,"100K7.5M","角パイプ100",71.400000000000006,3035,"MSO20","ミドルサポート下管",7.5,3179,"OKS-2","スペーストラス",null,4081,"SXBP15","採光防音パネル15",8.9,5140,"WA13","白シート（耳付き）",null,6065,"KSH1219","ハンドレール階段用",12.5,6279,"ALHCKP","アルミ梯子クランプ",0.5,6500,"ｳﾜﾔﾊﾟﾈﾙ４ｍ","上屋パネル４Ｍ",390,null,null,null,null,9019,3018,"メタルホーム",16.899999999999999]
[21,"A6155A","鳥居型建枠",11.8,123,"ALHT-N3","アルミハッチ付布板",8.5,null,null,null,null,358,null,null,null,516,"JFN-18","手摺1829",5,1077,"PJ14","ピポットジャッキ",4.5,2060,"100K8.0M","角パイプ100",61.9,3038,"MSI1C","Ｍサポート用クランプ",1.7,3180,"OKE-4","エンドトラスＬ３６５",null,4082,"SXBP12","採光防音パネル12",7.1,5145,"BM1851G","メッシュシート",5.3,6066,"CB1","キャッチベース",8.5,6280,"AL4M","アルミ梯子４Ｍ",10.4,6501,"ｳﾜﾔﾊﾟﾈﾙ８ｍ","上屋パネル８Ｍ",768,null,null,null,null,9020,3015,"メタルホーム",14.2]
[22,"A6117S","610建枠 H1700",11.8,124,"ALHT-N4","アルミハッチ付布板",9.6999999999999993,260,"ALAF-L","フレームＬ+斜材",10.7,359,null,null,null,null,null,null,null,1078,"CP20","建枠連結ピン",0.6,2061,"ｸｲﾏﾙ1.5","くい丸１．５ｍ",4,3039,"MSI2C","Ｍサポート用クランプ",1.8,3181,"OKA-R","アジャストトラス　右",null,4083,"SXBP09","採光防音パネル09",5.2,5146,"BM1551G","メッシュシート",4.4000000000000004,6067,"CB2","キャッチベース",9,6281,"AL6M","アルミ梯子６Ｍ",15.1,6502,"ﾄﾞｰﾑ　4M","採光ドーム４M",null,null,null,null,null,9021,3012,"メタルホーム",11.5]
[23,"A4517S","簡昜枠",10.7,125,"ALHT-N5","アルミハッチ付布板",11.4,261,"ALAF-R","フレームＲ+斜材",10.7,360,"FSJ-1","Ｆ支柱抜止ピン",null,530,"JFX-06","先行手摺筋違0610",3.6,1079,"A20ﾊﾞﾗ","連結ピン（バラピン）",0.6,2062,"ｸｲﾏﾙ1.1","くい丸１．１ｍ",3.6,3040,"MSO1C","Ｍサポート用クランプ",1.8,3182,"OKA-L","アジャストトラス　左",null,4084,"SXBP06","採光防音パネル06",3.4,5147,"BM1251G","メッシュシート",3.5,6068,"CB3","キャッチベース",9.5,6282,"AL6MS","アルミ２連梯子６Ｍ",19.2,6503,"ﾄﾞｰﾑ4M　ﾂｳﾛ","採光ドーム４M通路",null,null,null,null,null,9022,3009,"メタルホーム",8.8000000000000007]
[24,"A6112S","簡昜枠",0,126,"ALHT-H","アルミハッチ用梯子",4,262,"ALA18A","万能板受け（上）１８",4.5999999999999996,361,"FSJ-2","インナーロックピン",null,531,"JFX-09","先行手摺筋違0914",4.3,1080,"A100","連結ピン",0,null,null,null,null,3041,"MSO2C","Ｍサポート用クランプ",1.9,3183,"OKA-P","アジャストポスト",null,null,null,null,null,5148,"BM0951G","メッシュシート",2.6,6071,"M18","鉄馬",5,6283,"ＥＡＳＹＣＭ","イージークライマー",4.0999999999999996,6504,"ｳﾜﾔﾊﾟﾈﾙ4MK","上屋パネル４M開口",410,null,null,null,null,9023,3006,"メタルホーム",6.1]
[25,null,null,null,127,"NSH1700","垂直梯子",9.1,263,"ALA18B","万能押え１８２９",1.8,362,"CL30-OS","連結クランプ",0.7,532,"JFX-12","先行手摺筋違1219",5.0999999999999996,1081,"A20","連結ピン",0.6,null,null,null,null,3046,"CHI50","強力サポート（上管）",41.6,3184,"OKPB-6","調節ピン",null,5001,"A5×5N","安全ネット５ｍ*５ｍ",6.3,5149,"BM0751G","メッシュシート",2.1,6072,"M18S","スプリング鉄馬",10,6284,"SITA31","下さんｏｒ手摺 １８２９",1.8,6505,"ｳﾜﾔﾊﾟﾈﾙ8MK","上屋パネル８M開口",788,null,null,null,null,9024,2018,"メタルホーム",13.5]
[26,"A205","610調整枠 H1524",10.7,128,"SRTS","垂直梯子上段手摺",5,264,"ALA18D","万能板受け（下）１８",5,363,null,null,null,533,"JFX-15","先行手摺筋違1524",5.9,1082,"PCC","Ｃジョイント",0.74,null,null,null,null,3047,"CHI40","強力サポート（上管）",30,3185,"OKP-9","接続ピン",null,5002,"A6×6N","安全ネット６ｍ*６ｍ",9,5150,"BM0651G","メッシュシート",1.8,6073,"LBﾏｯﾄ","コンクリートマット",6.7,6285,"SITA32","下さんｏｒ手摺 １５２４",1.5,6506,"RB２ｶﾞﾀ","ルーフビーム２ｍ",100,7249,"ｳﾝﾊﾟﾝﾌﾟﾚｰﾄ","上屋運搬プレート",2,9025,2015,"メタルホーム",11.3]
[27,"A204","610調整枠 H1219",11.7,129,"HT-N6","鋼製ハッチ付布板",25,265,"ALA18C","振れ止め１８２９",2.1,364,null,null,null,534,"JFX-18","先行手摺筋違1829",6.8,1083,"PCJ","直線ジョイント 48.6⇔48.6",0.6,2066,"KK-1.5","鋼製杭１．５ｍ",4.2,3048,"CHI32","強力サポート（上管）",21.2,3186,"OKSP-9","スナップピン",null,5003,"A5×10N","安全ネット５ｍ*１０ｍ",12.5,5151,"BM1851BE","メッシュ（ベージュ）",5.3,6074,"ｽｷﾏｲﾀ４５０","隙間板４５０ｘ４５０",5,6286,"SITA29","下さんｏｒ手摺 １２１９",1.2,6507,"ﾄﾘﾂｹﾌﾟﾚｰﾄ","取付プレート",null,7250,"300H-12M","３００Ｈ型鋼１２ｍ",1128,9026,2012,"メタルホーム",9.1]
[28,"A203","610調整枠 H914",10.199999999999999,130,"ALHT-N6","アルミハッチ付布板",13.5,266,"ALAFK","フレーム受け金具",2.9,365,null,null,null,539,"JHBK-6","跳出ﾌﾞﾗｹｯﾄ610",5.2,1084,"SPJ","スプリングジョイント",0.7,2067,"P2C","同径自在クランプ",null,3049,"CHI24","強力サポート（上管）",12.5,3187,"OKEJ-1","エンドジョイント",null,5004,"A1×6N","安全ネット１ｍ*６ｍ",1.5,5152,"BM1551BE","メッシュ（ベージュ）",4.4000000000000004,6075,"ｽｷﾏｲﾀOS","スキマイタ",5,6287,"SITA27","下さんｏｒ手摺 ９１４",0.9,6508,"Ｒ３２＊３６","トルクレンチ",null,null,null,null,null,9027,2009,"メタルホーム",6.9]
[29,"A217","610調整枠 H490",7.5,131,"A2350","朝顔主材",15.6,267,"ALABB","ＦＲＰ製万能板",5,366,null,null,null,540,"JHBK-3","跳出ﾌﾞﾗｹｯﾄ305",4.4000000000000004,1085,"PEC","異形ジョイント 48.6⇔42.7",0.61,2068,"P1EC","異形直交クランプ",null,3050,"CHO16","強力サポート（下管）",27.8,3188,"OKJ-P","ジョイントピース",null,5005,"A3×6N","安全ネット３ｍ*６ｍ",4.5,5153,"BM1251BE","メッシュ（ベージュ）",3.5,6076,"ｽｷﾏｲﾀ","隙間板３７０×５７０",6.3,6288,"SITA28","下さんｏｒ手摺 ６１０",0.6,6509,"ﾚﾝﾌﾛｰｸﾗﾝﾌﾟ","レンフロークランプ",null,null,null,null,null,9028,2006,"メタルホーム",4.8]
[30,null,null,null,132,"A2006A","万能受Ｌ型",5.26,268,"ALA15A","万能板受け（上）１５",3.9,367,null,null,null,541,"JBKP-04","跳出ﾌﾞﾗｹｯﾄ400",2.6,1086,"BPCJL60K","６０角ジョイント",1.1200000000000001,2069,"P2EC","異形自在クランプ",null,3051,"CHD18","強力補助サポート",23.3,3189,"N．T（M42）","調節ピン用ナット",null,5006,"A8×8N","安全ネット８ｍ*８ｍ（青）",18,5154,"BM0951BE","メッシュ（ベージュ）",2.6,6077,"BKH４５３０","大型ブラケット",140,6289,"THR-912","妻側伸縮巾木",3.7,6510,"Ｒ３２ｿｹｯﾄ","ソケット３２",0.1,7260,"KS20-24","壁繋ぎ２００－２４０",null,9029,1518,"メタルホーム",9.5]
[31,null,null,null,133,"A2006B","万能押さえ",3.8,269,"ALA15B","万能押え１５２４",1.5,368,null,null,null,542,"JBKP-06","跳出ﾌﾞﾗｹｯﾄ600",3.3,1087,"BPCJL100K","１００角ジョイント",3,2070,"ARC1","直交クランプ兼用",0.7,3052,"CHD10","強力補助サポート",14.3,3190,"PW（M42)","調節ピン用PW",null,5007,"A10×10Ｎ","安全ネット１０ｍ*１０ｍ（グレー）",26,5155,"BM0651BE","メッシュ（ベージュ）",1.8,6078,"SGｽｷﾏｲﾀ","階段開口ｽｷﾏｲﾀ",2.8,6290,"CSR-130D","マイティー１３０型",13.2,6511,"ﾊﾟｲﾌﾟﾏﾝ（ｵﾈ","手摺金具",0.5,7261,"KS24-33","壁繋ぎ２４０－３３０",null,9030,1515,"メタルホーム",7.9]
[32,"A2617S","簡昜枠",12.7,134,"A2006D","万能受Ｃ型",5.8,270,"ALA15D","万能板受け（下）１５",4.0999999999999996,369,null,null,null,543,"JSBK-500","伸縮ﾌﾞﾗｹｯﾄ50",2.6,1089,"SD900カギ","ｻｲﾄﾞﾄﾞｱ・カギ",null,2071,"ARC2","自在クランプ兼用",0.7,3053,"CHSP","強力サポートピン",0,3191,"B-90","調節ピン用さらばね",null,5011,"R0.5×6N","ラッセルネット０.５ｍ*６ｍ",0.9,null,null,null,null,6079,"BKH4030","大型ブラケット",125,6291,"CSR-150D","マイティー１５０型",16.100000000000001,null,null,null,null,7262,"KS28-40","壁繋ぎ２８０－４００",null,9031,1512,"メタルホーム",6.4]
[33,null,null,null,135,"A2306C","振れ止",2.1,271,"ALA15C","振れ止め１５２４",1.9,370,"ｾｰﾌﾜｸ610","Ｆ先行手摺０６",6.3,544,"JSBK-750","伸縮ﾌﾞﾗｹｯﾄ75",3.7,1090,"SD900","ｻｲﾄﾞﾄﾞｱ９００",64,2072,"P3C","三連自在クランプ",1.1000000000000001,3056,"CHCU","ＣＨ－用根がらみ　小",3.78,3192,"HAND POMP","油圧手動ポンプ",null,5012,"R1×6N","ラッセルネット１ｍ*６ｍ",1.8,5200,"BM1851NS","メッシュ（グレー１㍉",5.3,6080,"BKH4536A","大型ブラケット",125,6292,"CSRR131","１００／１３０用手摺",6.9,6513,"ﾄﾞｰﾑﾊﾊﾞｶﾅ","ドーム巾調整金具",null,7263,"KS30-44","壁繋ぎ３００－４４０",null,9032,1509,"メタルホーム",4.9000000000000004]
[34,"A2","梯子型建枠",16.5,136,"BB623","万能板",12.2,272,"ALA12A","万能板受け（上）１２",3.2,371,"ｾｰﾌﾜｸ914","Ｆ先行手摺０９",8.1999999999999993,545,"JSBK-1000","伸縮ﾌﾞﾗｹｯﾄ100",5.0999999999999996,1091,"SSK200","安全鋼板",12,2073,"P3CC","三連直交クランプ",1.1000000000000001,3057,"CHCD","ＣＨ－用根がらみ　大",4.05,3193,"ﾊﾟﾜｰｼﾞｬｯｷ","油圧ジャッキ",null,5013,"R2×6N","ラッセルネット２ｍ*６ｍ",3.6,5201,"BM1551NS","メッシュ（グレー１㍉",4.4000000000000004,6081,"BKH4536B","大型ブラケット",125,6293,"CSRR161","１５０型用手摺",7.3,6514,"ｳﾜﾔﾊﾟﾈﾙ６ｍ","上屋パネル６Ｍ",576,7264,"KS32-48","壁繋ぎ３２０－４８０",null,9033,1506,"メタルホーム",3.4]
[35,"A2S","梯子型調節枠",9.9,137,"A2006A-15","万能受Ｌ型 1500用",4.4000000000000004,273,"ALA12B","万能押え１２１９",1.3,372,"ｾｰﾌﾜｸ1219","Ｆ先行手摺１２",9.1999999999999993,546,"JBKN-04","ﾌﾞﾗｹｯﾄ400",2.1,1092,"SSK200(ｲﾛ)","安全鋼板（色付き）",12,2074,"KMP1C","６０角丸クランプ直交",0.77,3058,"40ｶﾞﾀK","強力サポート　Ｋ",58,3194,"OKSR-450","OKスピードローラー",null,5014,"R3×6N","ラッセルネット３ｍ*６ｍ",5.4,5202,"BM1251NS","メッシュ（グレー１㍉",3.5,6082,"ｽｷﾏｲﾀ240","隙間板２４０ｘ４５０",3.5,6294,"LT-14","ラクラクタラップ１４",14,6515,"ｼｬｺﾏﾝBE50M","シャコ万力",null,7265,"KS42-59","壁繋ぎ４２０－５９０",null,9034,1018,"メタルホーム",7.7]
[36,"A15R","手摺枠",10.6,138,"A2006B-15","万能押さえ 1500用",3.2,274,"ALA12D","万能板受け（下）１２",3.2,373,"ｾｰﾌﾜｸ1524","Ｆ先行手摺１５",11,null,null,null,null,1093,"SSK300","安全鋼板",18,2075,"KMP2C","６０角丸クランプ自在",0.77,3059,"24ｶﾞﾀK","強力サポート　Ｋ",40.1,3195,"ﾍﾞｰｽﾌﾟﾚｰﾄ","SR用ベースプレート",null,5015,"R5×5N","ラッセルネット５ｍ*５ｍ",7.5,5203,"BM0951NS","メッシュ（グレー１㍉",2.6,null,null,null,null,6295,"LT-24","ラクラクタラップ２４",21,6516,"ﾄﾞｰﾑｶﾅｸﾞ6M","ドーム巾調整金具６M",null,7266,"KS48-67","壁繋ぎ４８０－６７０",null,9035,1015,"メタルホーム",6.4]
[37,"A15RD","手摺枠扉付",11.7,139,"A2006D-15","万能受Ｃ型 1500用",4.8,275,"ALA12C","振れ止め１２１９",1.7,374,"ｾｰﾌﾜｸ1829","Ｆ先行手摺１８",11.9,550,"JHL-2","梁枠2ｽﾊﾟﾝ用",23.9,1094,"SSK300P","パンチング鋼板",18,2076,"KKP1C","６０角角クランプ直交",0.88,3060,"CHD12K","強力補助サポート　Ｋ",null,3196,"OKSR-P","OKSR用鎖ピン",null,5016,"R6×6N","ラッセルネット６ｍ*６ｍ",10.8,5204,"BM0751NS","メッシュ（グレー１㍉",null,6106,"ﾂﾘｶﾅｸﾞ","法面足場　吊り金具",1,6296,"LT-38","ラクラクタラップ３８",35,6517,"ﾄﾞｰﾑ 2M","採光ドーム２Ｍ",null,7267,"KS57-86","壁繋ぎ５７０－８６０",null,9036,1012,"メタルホーム",5.2]
[38,null,null,null,140,"A2306C-15","振れ止 1500用",1.7,276,"ALA09A","万能板受け（上）０９",2.5,375,"FX-06","ﾌｭｰｼﾞｮﾝ先行手摺06",4.3,551,"JHL-3","梁枠3ｽﾊﾟﾝ用",35.5,1095,"SSK300(ｲﾛ)","安全鋼板（色付き）",18,2077,"KKP2C","６０角角クランプ自在",0.88,3061,"SSH300","四角支柱３．００Ｍ",54.4,3197,"ｿｹｯﾄﾚﾝﾁ","ソケットレンチ",null,5017,"R5×10N","ラッセルネット５ｍ*１０ｍ",15,5205,"BM0651NS","メッシュ（グレー１㍉",1.8,6107,"CAT-HG・P50","法面足場ハンガー５０丸用",1,6297,"LTT-14","ラクタラップ１４手摺",4,6518,"ｳﾜﾔﾃｽﾘﾊﾟｲﾌﾟ","上屋用手摺パイプ",null,7268,"KS67-86","壁繋ぎ６７０－８６０",null,9037,1009,"メタルホーム",3.9]
[39,null,null,null,141,"A2006A-12","万能受Ｌ型 1200用",3.5,277,"ALA09B","万能押え９１４",1,376,"FX-09","ﾌｭｰｼﾞｮﾝ先行手摺09",4.9000000000000004,559,"JOBTK","大組払し専用吊り金具",3,1096,"SSK300(ｸﾘｱ）","クリアフェンス",4.4000000000000004,2078,"KMARC1","６０角ｘ兼用直交",0.9,3062,"SSH225","四角支柱２．２５Ｍ",45.2,3198,"ｿｹｯﾄ32","ソケット３２",null,5018,"R8×8N","ラッセルネット８ｍ*８ｍ",19.2,5210,"A3X6NS","安全ネット",null,6108,"ｷｬｯﾄｳｫｰｸ","法面足場　本体",12,6298,"LTT-24","ラクタラップ２４手摺",6.2,6519,"ｲｰｸﾞﾙｸﾗﾝﾌﾟ","イーグルクランプ",4,7269,"KS86-105","壁繋ぎ８６０－１０５０",null,9038,1006,"メタルホーム",2.7]
[40,null,null,null,142,"A2006B-12","万能押さえ 1200用",2.5,278,"ALA09D","万能板受け（下）０９",2.2000000000000002,377,"FX-12","ﾌｭｰｼﾞｮﾝ先行手摺12",5.7,560,"JFT-PIN","JFT連結ﾋﾟﾝ",0.5,1097,"ﾌﾗｯﾄﾊﾟﾈﾙ３ｍ","フラットパネル　３Ｍ",18,2079,"KMARC2","６０角ｘ兼用自在",0.9,3063,"SSH200","四角支柱２．００Ｍ",41.1,3199,"ｿｹｯﾄ41","ソケット４１",null,5020,"G5×7N","グリーンネット５ｍ*７ｍ",null,5211,"A5X5NS","安全ネット",null,6109,"CAT-HG・K60","法面足場ハンガー６０角用",1,6299,"LTBA-6","ラク２ベース金具",4.5,6520,"Kﾌﾚｰﾑ4M","開口フレーム４ｍ",null,7270,"NBS200","ブラケットサポート",null,9039,"GJ","ガッチリジョイント",0.7]
[41,"OB6109","支保工枠",14.3,143,"A2006D-12","万能受Ｃ型 1200用",3.9,279,"ALA09C","振れ止め９１４",1.6,378,"FX-15","ﾌｭｰｼﾞｮﾝ先行手摺15",6.5,561,"SH-120","カラー材",0.3,1098,"ﾌﾗｯﾄｺｰﾅｰ３Ｍ","フラットコーナー３Ｍ",8,2080,"BH","ボードホルダー",0.6,3064,"SSH125","四角支柱１．２５Ｍ",30.5,3200,"ｿｹｯﾄ65","ソケット６５",null,5021,"G5×10N","グリーンネット５ｍ*１０ｍ",7.5,5212,"A5X10NS","安全ネット",null,6110,"F・ｱｼﾊﾞｲﾀ","＊＊ＦＳ用Ｓ足場板",null,6300,"ＳＳＫＦＢＨ","フックボルト",null,6521,"Kﾌﾚｰﾑ1.4M","開口フレーム１．４ｍ",null,7271,"NBO140","ブラケットサポート",null,9040,"CG1206","妻手摺"]
[42,"OB9109","支保工枠",19.3,144,"A2306C-12","振れ止 1200用",1.4,280,"ALA06A","万能板受け（上）０６",1.8,379,"FX-18","ﾌｭｰｼﾞｮﾝ先行手摺18",7.4,563,"CL66-OS","ﾂﾅｷﾞｸﾗﾝﾌﾟ",0.9,1099,"ﾌﾗｯﾄﾊﾊﾞ３Ｍ","フラット巾調整３Ｍ",15.5,2081,"AKBP","筋交い止めクランプ",0.4,3065,"SSH65","四角支柱０．６５Ｍ",23,3201,"KP130-1.0M","角パイプ７０×１３０",6.95,5022,"G6×10N","グリーンネット６ｍ*１０ｍ",null,5213,"A6X6NS","安全ネット",null,6111,"F・ﾇﾉｲﾀ","＊＊ＦＳ用パイプ付布",null,6301,"GB","ゴムバンド",null,6522,"R30ｿｹｯﾄ","ソケット ３０",0.1,null,null,null,null,9041,"KS-130","壁つなぎ"]
[43,"OB4512","支保工枠",14.5,145,"A2006A-09","万能受Ｌ型 900用",2.6,281,"ALA06B","万能押え６１０",0.8,382,"FA-0862PN","ピン無し支柱862",4.2,570,"JAL457","ｱﾙﾐ階段1818",12.4,1100,"ｾﾝﾖｳﾗｯｸ","専用ラック",7.7,2082,"100KMP1C","100角×兼用 直交",1.6,3066,"SSJ58F","自在ジャッキ",32.6,3202,"KP130-1.5M","角パイプ７０×１３０",10.43,5023,"G7×10N","グリーンネット７ｍ*１０ｍ",10.5,5214,"A8X8NS","安全ネット",null,6112,"F・ﾀﾃﾜｸ","＊＊ＦＳ用折タタミ枠",null,6302,"HTB(12mm)","ﾊｲﾃﾝｼｮﾝﾎﾞﾙﾄ１２",null,6988,"Rﾊﾟﾚﾃｰﾅ","レンタルパレテーナ",null,7275,"ｽｷﾏ45*65","隙間板４５０＊６５０",null,9042,"QB624","クイックボード",8.1]
[44,"OB4509","支保工枠",12.1,146,"A2006B-09","万能押さえ 900用",1.9,282,"ALA06D","万能板受け（下）０６",1.4,390,"PAM-S","Fパレット小",null,571,"JSG918","階段開口部手摺枠",13.4,1101,"ﾌﾗｯﾄﾊﾟﾈﾙ２ｍ","フラットパネル　２Ｍ",12,2083,"100KMP2C","１００角丸クランプ",1.6,3067,"SSJ58","固定ジャッキ",32.6,3203,"KP130-2.0M","角パイプ７０×１３０",13.9,5024,"BM0651KG","メッシュ(グレー）",1.8,5215,"A10X10NS","安全ネット",null,6113,"Ｆ・ｼﾞｬｯｷﾍﾞｰｽ","＊＊ＦＳ用Ｊベース",null,6303,"HTB(16mm)","ﾊｲﾃﾝｼｮﾝﾎﾞﾙﾄ１６",null,6989,"ｳﾝﾊﾟﾝBOX","運搬BOX",null,7276,"ｽｷﾏｲﾀ50x70","隙間板５００＊７００",null,9043,"QBC","クイッククランプ",2]
[45,"OB4504","支保工枠",8.5,147,"A2006D-09","万能受Ｃ型 900用",2.9,283,"ALA06C","振れ止め６１０",1.4,391,"PAM-L","Fパレット大",null,572,"JSU2X","階段斜め手摺",5,1102,"ﾌﾗｯﾄｺｰﾅｰ２Ｍ","フラットコーナー２Ｍ",5,null,null,null,null,3068,"SSF75","**自在ベース",null,3204,"KP130-2.5M","角パイプ７０×１３０",17.399999999999999,5025,"BM0751KG","メッシュ(グレー）",2.1,5220,"R0.5X6NS","ラッセルネット",null,6114,"ﾏﾙﾁｽﾃｰｼﾞ","マルチステージ",47,6304,"HTB(20mm)","ﾊｲﾃﾝｼｮﾝﾎﾞﾙﾄ２０",null,6990,"ﾊﾟﾚﾃｰﾅ","パレテーナ",null,7277,"MA143","２スパン梁枠",null,9044,"A8×8N","安全ネット"]
[46,"A9117","ブラケット枠",16,148,"A2306C-09","振れ止 900用",1.1000000000000001,284,"ALACF-L","隅フレームＬ",9.5,null,null,null,null,573,"JNU-123","階段受け1219",4,1103,"ﾌﾗｯﾄﾊﾊﾞ２Ｍ","フラット巾調整２Ｍ",10.5,null,null,null,null,3069,"SSU31","梁受金具",11,3205,"KP130-3.0M","角パイプ７０×１３０",20.85,5026,"BM0951KG","メッシュ(グレー）",2.6,5221,"R1X6NS","ラッセルネット",null,6115,"ｱﾀｯﾁﾒﾝﾄ","＊＊Ｍアタッチメント",null,6305,"RNETKH","ネット結束糸",null,6991,"ｶﾞﾝﾊﾞｺ（Ｍ）","ガンバコ（Ｍ）",null,7278,"MA147","３スパン梁枠",null,9045,"ﾉﾘﾒﾝｱｼﾊﾞ","法面足場"]
[47,"A2617","ブラケット枠",19,149,"KONA6-0912","調節万能Ｃ受け(小）",null,285,"ALACF-R","隅フレームＲ",9.5,null,null,null,null,574,"JNU-093","階段受け0914",3.6,1104,"ﾄﾞｱﾊﾟﾈﾙ","ドアパネル",17.899999999999999,2087,"CKP1(H)","鉄骨クランプ直行座付",1.05,3071,"NSJ30","頭部専用ジャッキ",35.200000000000003,3206,"KP130-3.5M","角パイプ７０×１３０",24.33,5027,"BM1251KG","メッシュ(グレー）",3.5,5222,"R2X6NS","ラッセルネット",null,null,null,null,null,6306,"BMKH","メッシュ結束糸",null,6992,"TOWERD-26","タワード２６",227,null,null,null,null,9052,"ﾉﾘﾒﾝﾌﾞﾗｹｯﾄ","法面ブラケット",3.5]
[48,"A6117","ブラケット枠",15,186,"KONA1-AR","隅朝顔本体　右",15,286,"ALACF-C","隅フレームＣ",19.100000000000001,392,"FXﾊﾟﾚｯﾄ","ＦＸパレット",75,575,"ＪＮＵ-063","階段受け0610",2.9,1105,"ﾄﾞｱｼﾞｮｳﾌﾞ","ドアパネル上部",1,2088,"CKP2(H)","鉄骨クランプ自在座付",1.05,3081,"22AT1225","敷鉄板",null,3207,"KP130-4.0M","角パイプ７０×１３０",27.8,5028,"BM1551KG","メッシュ(グレー）",4.4000000000000004,5223,"R3X6NS","ラッセルネット",null,null,null,null,null,6307,"G-BMKH","グレーメッシュ結束糸",null,6993,"ﾊﾟﾚｯﾄＭ","パレット（Ｍ）",null,7280,"DB-TEPA","電動ブレーカキャップ",2.4,9053,"SKN2","鋼製布板",7.2]
[49,"A4561","ブラケット枠",17.399999999999999,187,"KONA2-AC","隅朝顔本体　中",18,287,"ALAC4","隅万能板押え",2.2999999999999998,393,"FXｼﾁｭｳ1","ＦＸシチュウ中間柱左",7.8,580,"JOSK-C1","養生クランプロング",0.5,1106,"ﾒｯｼｭﾊﾟﾈﾙ3M","メッシュパネル３Ｍ",17.899999999999999,2089,"CKPM(H)","鉄骨マルチ座付",1.05,3082,"22AT1530","敷鉄板",802,3208,"KP130-4.5M","角パイプ７０×１３０",31.3,5029,"BM1851KG","メッシュ(グレー）",5.3,5224,"R5X5NS","ラッセルネット",null,6200,"MS40","上屋パネル２．３×４",null,6308,"WSKH","結束糸（白）",null,6994,"ツリパレット","吊パレット",101,7281,"AB-30","エアブレーカキャップ",1.8,9054,"BKN224","鋼製布板",4.5999999999999996]
[50,"SKR6","ローリング用鋼製布板",15.9,188,"KONA3-AL","隅朝顔本体　左",15,288,"ALAC5","振れ止め　Ａ",1.7,394,"FXｼﾁｭｳ2","ＦＸシチュウ中間柱右",7.8,581,"JOSK-C3","三爪クランプロング",0.6,1107,"ﾌﾗｯﾄｸﾘｱ3M","フラットクリア３Ｍ",6.6,2090,"CKP-M","鉄骨クランプマルチ",1.05,3083,"22AT1560","敷鉄板",1604,3209,"KP130-5.0M","角パイプ７０×１３０",34.799999999999997,5030,"OZ06Y","親綱 ６Ｍ(青)",1.02,5225,"R5X10NS","ラッセルネット",null,6201,"MS60","上屋パネル２．３×６",null,null,null,null,null,6995,"WK-150","吊パレ用キャスター",3,null,null,null,null,9056,"100KKMP1C","100角丸ｸﾗﾝﾌﾟ（直）"]
[51,"SKN6","1829布板",15.9,189,"KONA4-R","隅万能板　右",30,289,"ALAC6","振れ止め　Ｂ",1.9,395,"FXｱﾝｸﾞﾙ","ＦＸパレットアングル",null,582,"JOSK-A1","養生クランプ板付",1,1108,"ﾒｯｼｭﾊﾟﾈﾙ2M","メッシュパネル２Ｍ",12,2091,"NKMIP","手摺クランプ（垂直）",0.95,3084,"22AT1530M","敷鉄板（未整備）",802,3210,"KP130-5.5M","角パイプ７０×１３０",38.25,5031,"OZ10","親綱１０Ｍ（グレー）",1.7,5226,"R6X6NS","ラッセルネット",null,6210,"ALV11","アルバステップ本体",12,null,null,null,null,6996,"WJ-150S","吊パレキャッスタ輪止付",3,null,null,null,null,9157,"H-150 4.0M","Ｈ鋼４．０Ｍ",126]
[52,"SKN5","1524布板",13.5,190,"KONA5-L","隅万能板　左",30,290,"ALACFK","隅フレーム受け金具",9.5,null,null,null,null,583,"JOSK-A3","三爪クランプ板付",1.5,1109,"ﾌﾗｯﾄｸﾘｱ2M","フラットクリア２Ｍ",4.4000000000000004,2092,"NKMI","手摺クランプ（水平）",0.95,3085,"22AT1560M","敷鉄板（未整備）",1604,3211,"KP130-6.0M","角パイプ７０×１３０",41.7,5032,"OZ15","親綱１５Ｍ（緑）",2.6,5227,"R7X7NS","ラッセルネット",null,6211,"ALVR11","アルバステップ手摺",6.4,6311,"1.0m（打込み）","打込みパイプ１ｍ販売",2.73,6997,"ﾈｯﾄﾖｳﾊﾟﾚﾃﾅ","ネット用特注パレテナ",4,null,null,null,null,9158,"H-150 6.0M","Ｈ鋼６．０Ｍ",189]
[53,"SKN4","1219布板",11.1,191,"KONA6","調節万能Ｃ受け",6.5,291,"ALACB1","ＦＲＰ製万能板　小",3,400,"VS-1","ベランダステップ本体",null,null,null,null,null,1110,"ﾄﾞｱﾊﾟﾈﾙ１ｍ","ドアパネル１ｍ",38.5,2093,"FNKMIP","手摺クランプ（垂直）",0.95,3091,"RMT・ＪＴ","ジョイントパイプ",0,null,null,null,null,5033,"OZ20","親綱２０Ｍ（黒）",3.4,5228,"R8X8NS","ラッセルネット",null,6219,"THR-6","610枠用妻側巾木",2.1,6312,"1.5m（打込み）","打込みパイプ１．５ｍ販売",4.0999999999999996,null,null,null,null,7290,"A8x9N","安全ネット",null,9159,"H-150 1.5M","Ｈ鋼１．５Ｍ",47.3]
[54,"SKN3","914布板",8.9,192,"KONA7","方杖ＫＣ－１８",7,292,"ALACB2","ＦＲＰ製万能板　中",5,401,"VS-T","ベランダステップ手摺",null,null,null,null,null,1111,"DﾊﾟﾈﾙｶｷﾞA","ドアパネル鍵",null,2094,"FNKMI","手摺クランプ（水平）",0.95,3092,"RMT","ロードマット",6.7,4001,"P5","ペコービーム内",14.4,5035,"OZ30","親綱３０Ｍ",5.0999999999999996,null,null,null,null,6220,"ST-1","先行手摺り用固定金具",3.6,6313,"WS1551","白シート 1524*5100",4.4000000000000004,null,null,null,null,7291,"0.5x6NB","０．５Ｒネット（青）",null,9160,"H-150 2.0M","Ｈ鋼２．０Ｍ",63]
[55,"SKN2","610布板",5.5,193,"ｸﾗﾝﾌﾟ1P","隅朝顔",0.6,293,"ALACB3","ＦＲＰ製万能板　大",8,402,"VS-2","ベランダS補助梯子",null,null,null,null,null,1112,"DﾊﾟﾈﾙｶｷﾞB","ドアパネル１M鍵",null,2095,"ｱﾝｸﾗﾝﾌﾟC-1","アンクランプＣ型直行",1.5,null,null,null,null,4002,"P9","ペコービーム内",28,5036,"WS13","白シート(中古）",5.3,5231,"OZ10NS","親綱１０Ｍ（青）",1.7,6221,"ST-2","先行手摺り手摺り柱",5.8,6314,"WS1251","白シート 1219*5100",3.5,null,null,null,null,null,null,null,null,9266,"SSHBNT","四角支柱ボルト・ナット",0.21]
[56,"SKN-400","鋼製布板",13,194,"ｸﾗﾝﾌﾟ2P","隅朝顔",1,294,"ALATFK","妻側フレーム受け金具",3,403,"VS-SH","ベランダS水平材",null,null,null,null,null,1147,"OSA27","下さん９１４",0.9,2096,"ｱﾝｸﾗﾝﾌﾟC-2","アンクランプＣ型自在",1.5,3100,"OKSS-2","ＯＫ支柱２１５",1.8,4003,"L5","ペコービーム外",16.7,5037,"WS12","白シート",3.5,5232,"OZ15NS","親綱１５Ｍ（黄色）",2.6,6222,"ST-3","先行伸縮手摺",2.9,6315,"WS0951","白シート 914*5100",2.6,null,null,null,null,null,null,null,null,9267,"BMKH(B)","結束し"]
[57,"BKN624","1829布板ハーフ",9,195,"ｸﾗﾝﾌﾟ3P","隅朝顔",1.4,295,"ALA7XJ","主材受金具（次世代用",2.9,404,"VS-TW","ベランダS手摺枠",null,null,null,null,null,1148,"OSA28","下さん６１０",0.6,2097,"CKP1","キャッチクランプ直交",1.1000000000000001,3101,"OKSS-4","ＯＫ支柱４３１",2.7,4004,"L7","ペコービーム外",20.399999999999999,5038,"WS13K","白シート(新品)",5.3,5233,"OZ20NS","親綱２０Ｍ（赤）",3.4,6223,"ST-4","先行伸縮手摺",5.5,6316,"WS0651","白シート 610*5100",1.8,7003,"ＢＳ－０１０","スタンドバリケード",null,null,null,null,null,9269,"RNETKH","結束し"]
[58,"BKN524","1524布板ハーフ",7.8,196,"ｸﾗﾝﾌﾟ1PBP","１ＰｸﾗﾝﾌﾟＢＰ用",0.7,296,"ALAC7XJS","隅受金具（次世代用",9.5,null,null,null,null,null,null,null,null,1149,"OSA29","下さん１２１９",1.2,2098,"CKP2","キャッチクランプ自在",1.1000000000000001,3102,"OKSS-8","ＯＫ支柱８６２",4.4000000000000004,4005,"L9","ペコービーム外",25.6,5041,"BM0651","メッシュシート610巾",1.8,5240,"G6X6NS","垂直ネット",null,6224,"FSPR-06","先行手摺 ０６",4.8,6317,"ﾋｷﾖｾﾛｰﾌﾟ","引寄ロープ",null,null,null,null,null,null,null,null,null,9270,"BMKH(G)","結束し"]
[59,"BKN424","1219布板ハーフ",6.6,197,"ｸﾗﾝﾌﾟ2PBP","２ＰクランプＢＰ用",0.8,300,"FA-0216","支柱 H=２１６",2,410,"SD60*80","スイングドア",5.5,null,null,null,null,1150,"OSA31","下さん１８２９",1.8,2099,"CKP1-W","手摺クランプ兼用固定",1.1000000000000001,3103,"OKSS-17","ＯＫ支柱１７２５",8.3000000000000007,4006,"ｺｳﾗﾝﾋﾞｰﾑ","高欄ビーム２０００",14.5,5042,"BM0751","メッシュシート",2.1,5241,"G6X12NS","垂直ネット",null,6225,"ASGF-18T","アルミスカイガード",null,6318,"ｸﾘｱｼｰﾄ","クリアシート",3.3,7005,"ＧＦ１８１８","ガードフェンス",null,null,null,null,null,9271,"SSKFBH","フックボルト",0.06]
[60,"BKN324","914布板ハーフ",5.5,198,"ｸﾗﾝﾌﾟ3PBP","３ＰクランプＢＰ用",2.1,301,"FA-0431","支柱 H=４３１",2.7,411,"DR-9","侵入防止扉",21,null,null,null,null,1151,"OSA32","下さん１５２４",1.5,2100,"CKP2-W","手摺クランプ兼用自在",1.1000000000000001,3104,"OKSH-6","水平ブレス６１０Ｌ",2.1,4007,null,null,null,5043,"BM0951","メッシュシート914巾",2.6,5242,"G6X15NS","垂直ネット",null,6226,"ASGF-15T","アルミスカイガード",null,6319,"Ｊフック","Ｊフック",0.1,7006,"GF1818E","ガードフェンス絵入り",17,null,null,null,null,9272,"GB","ゴムバンド"]
[61,"SS624","セフティーガードバン",8.3000000000000007,199,"YｼﾞｸﾗﾝﾌﾟBP","Ｙ字クランプＢＰ用",0.7,302,"FA-0862","支柱 H=８６２",4.5,412,"DR-9ｶｷﾞ","侵入防止扉用鍵",null,1001,"A14","筋違　（橙）",4.2,null,null,null,null,2101,"NRH1","ロックマン",2.98,3105,"OKSH-9","水平ブレス９１４Ｌ",2.8,null,null,null,null,5044,"BM1251","メッシュシート1219巾",3.5,5250,"NSﾛｯｸ","親綱緊張器",null,6227,"ASGF-12T","アルミスカイガード",null,6320,"D2ｶﾅｸﾞ","Ｄ２金具",0.1,7007,"ベース","フェンスベース",null,null,null,null,null,9273,"HTB","ハイテンションボルト"]
[62,"ＳＳ２４","アームクランプ",3.8,200,"OA-2390R","SKアサガオ主材（右",null,303,"FA-1725","支柱 H=１７２５",6.9,null,null,null,null,1002,"A11","筋違　（黄）",3.7,null,null,null,null,2102,"NCK 8t","チャック金物８ｔ用",2,3106,"OKSH-12","水平ブレス１２１９Ｌ",3.5,4008,"ｽﾃｰｼﾞｸﾗﾝﾌﾟ","ステージクランプ",null,5045,"BM1551","メッシュシート1524巾",4.4000000000000004,5251,"NSP NS","親綱支柱",null,6228,"ASGF-09T","ALスカイガード",null,6321,"D1ｶﾅｸﾞ","ジョイント金具コーナ",null,null,null,null,null,7465,"L4000(KK","鋼製足場板４ｍ",null,9274,"SSKFBH(ﾁｭｳｺ）","フックボルト",0.06]
[63,"BKN224","610布板ハーフ",3.5,201,"OA-2390L","SKアサガオ主材（左",null,304,"FA-3450","支柱 H=３４５０",12.8,420,"SF-09S","パイプハシゴ０９",6.8,1003,"A13","筋違　（黒）",3.3,null,null,null,null,2103,"ﾌﾞﾙﾏﾝ","ブルマン",2.98,3107,"OKSH-15","水平ブレス１５２４Ｌ",4.3,4010,"ｱﾀｯﾁﾒﾝﾄ","取付アタッチメント",0.3,5046,"BM1851","メッシュシート1829巾",5.3,5300,"JRG15OA","安全ブロック１５ｍ",6.4,6229,"K-1W","抱合せ部据え置き金具",null,6322,"M20*55","上屋ボルト・プレート",null,7018,"ｽﾁｰﾙﾍﾞｰｽ用ｶｺﾞ","ベース用カゴ"]
[64,"AL3055S","アルミ階段",10,202,"OA-3000S","SKアサガオ斜材",null,305,"FA-2587","支柱 H=２５８７",10,421,"SF-18S","パイプハシゴ１８",12.9,1004,"A012","筋違　（緑）",2.9,2000,"0.8M","丸パイプ",2.2000000000000002,2104,"Hｸﾗﾝﾊﾟｰ","Ｈクランパー",0.7,3108,"OKSH-18","水平ブレス１８２９Ｌ",5,4011,"SX14","軽量ビーム１４",14.7,5047,"OZ8Y","親綱８Ｍ(赤)",1.4,5301,"M-15ｶﾞﾀ","マイブロック１５ｍ",4.2,6230,"FSPR-18","先行手摺 １８",7.4,6323,"ﾊﾟｲﾌﾟﾏﾝ","パイプマン",null,7019,"ｶﾞｰﾄﾞﾌﾞﾛｯｸ","ガードブロック",9,7551,"ｼｮｰﾄﾋﾞｰﾑ(借)","HB095",8,9277,"コマイタ","コマイタ"]
[65,"K3012S","階段枠１２スパン用",21.1,203,"OA-08S","SKアサガオ斜材S管",null,306,null,null,null,422,"SF-27S","パイプハシゴ２７",19.2,1005,"A12","筋違　（青）",2.6,2001,"0.5M","丸パイプ",1.37,2105,"ｶﾞｰﾄﾞｸﾗﾝﾌﾟ","ガードクランプ",1.5,3109,"OKSB1710","筋違１７１０",5.3,4012,"SX22","軽量ビーム２２",24.7,5048,"OZ10Y","親綱１０Ｍ(灰)",1.7,null,null,null,null,6231,"Ｋ-２","先行金具 (先送用)",1.7,6325,"ﾄﾞｰﾑｼｰﾄ","ドームシート",null,null,null,null,null,null,null,null,null,9278,"バタカク","バタ角"]
[66,"K3055S","階段枠",25,204,"OA-UK","主材取付金具 BN付",null,307,null,null,null,423,"SF-36S","パイプハシゴ３６",24.8,1006,"A19","筋違　（灰）",3.9,2002,"0.6M","丸パイプ",1.64,2106,"AC20","チェーン２Ｍ",1.2,3110,"OKSB2318","筋違２３１９",6.7,4014,"SX454","軽量ビーム４５４",0,5049,"OZ15Y","親綱１５Ｍ(緑)",2.6,null,null,null,null,6232,"FSPR-15","先行手摺 １５",6.7,6326,"ﾄﾞｰﾑｼｰﾄﾂｳﾛ","ドームシート通路用",null,7026,"ﾌｪﾝｽｸﾗﾝﾌﾟ","フェンスクランプ",null,7607,"A8×8N（ｓ）","安全ﾈｯﾄ（ｓ）",null,9279,"ﾊﾞﾀｶｸ2.0ｍ","バタ角２.０Ｍ"]
[67,"K4055S","階段枠",36.200000000000003,205,"OA-PK","斜材取付金具 BN付",null,308,null,null,null,424,"ｾｶｺﾞ700","背カゴ",16,1007,"A18","筋違　（赤）",3.4,2003,"0.7M","丸パイプ",1.92,2107,"AC30","チェーン３Ｍ",1.8,3111,"OKSB931","筋違９３１",2.2000000000000002,4015,null,null,null,5050,"OZ20Y","親綱２０Ｍ(黒)",3.4,null,null,null,null,6233,"FSPR-12","先行手摺 １２",6.1,6327,"ﾄﾞｰﾑｼｰﾄﾂﾏ","ドームシート妻側用",null,null,null,null,null,7642,"1.5M(N","丸パイプ日建"]
[68,"K4064S","階段枠",47,206,"OA-2306A","SKバンノー受 L型",null,309,null,null,null,null,null,null,null,1008,"A07","筋違　（黒）",2.4,2004,"0.9M","丸パイプ",2.46,2108,"AC40","チェーン４Ｍ",2.4,3112,"OKS-A752","ＯＫＳジャッキベース",4,4016,"HB095","ホリービーム",8,5051,"BM0651OG","メッシュシート610巾",1.8,null,null,null,null,6234,"FSPR-09","先行手摺 ０９",5.4,6329,"M20*70","上屋ボルト・エンド",null,null,null,null,null,7643,"ｲｰｼﾞｰｸﾗｲﾏｰｻｲﾄﾞﾌﾟﾚｰﾄ（ｓ）","ｲｰｼﾞｰｸﾗｲﾏｰｻｲﾄﾞﾌﾟﾚｰﾄ（ｓ）",null,9308,"GF18ﾄﾋﾞﾗ（S","ガードフェンス１８扉（仙台"]
[69,"K3015S","階段枠１５スパン用",23.6,207,"OA-2306D","SKバンノー受 C型",null,310,"FC-0150","手摺 L=１５０",0.7,null,null,null,null,1009,"A09","筋違　（橙）",2.1,2005,"1.0M","丸パイプ",2.73,2109,"NRH-1（ミニ）","ミニロックマン",0.6,3113,"OKS-A752-H","ＯＫＳ大引受ジャッキ",5.4,4020,"HB454","ホリービーム",43,5052,"BM0751OG","メッシュシート",2.1,6002,"G2820S","敷板２Ｍ",9,6235,"K-1","先行金具 (据置用)",1.3,6330,"BEBMKH","ﾍﾞｰｼﾞｭ結束糸",null,7093,"ＰＧ－６３","パネルゲート",null,7644,"ｲｰｼﾞｰｸﾗｲﾏｰ取付ﾊﾞｰ（ｓ）","ｲｰｼﾞｰｸﾗｲﾏｰ取付ﾊﾞｰ（ｓ）"]
[70,"SS1-1ｶﾞﾀ","自在ステップ６００巾",4.5,208,"OA-2306B","SKバンノー押え",null,311,"FC-0305","手摺 L=３０５",1,null,null,null,null,1010,"A08","筋違　（若緑）",3.7,2006,"1.2M","丸パイプ",3.28,2110,"NCK10t","チャック金物１０ｔ用",2,3114,"OKS-A752-W","ＯＫＳ大引受ジャッキ",0,4021,"SPﾋﾞｰﾑ（Ｒ）","スーパービーム　右",20.52,5053,"BM0951OG","メッシュシート914巾",2.6,6004,"G2840S","敷板４Ｍ",18,6236,"FHR-18","巾木１８ (橙)",4.4000000000000004,6331,"W1/2ﾅｯﾄ","Ｗ１／２ナット",null,null,null,null,null,7645,"3.0M(N","丸パイプ日建"]
[71,"SS1-3ｶﾞﾀ","自在ステップ６００巾",6,209,"OA-2306C","SKフレ止め",null,312,"FC-0610","手摺 L=６１０",1.9,null,null,null,null,1011,"A9","筋違　（白）",3.1,2007,"1.5M","丸パイプ",4.0999999999999996,2111,"TB3","ターンバックル",0.3,3115,"OKSBP-1","支柱抜け止めピン",0.1,4022,"SPﾋﾞｰﾑ（Ｌ）","スーパービーム　左",20.52,5054,"BM1251OG","メッシュシート1219巾",3.5,6007,"G2820","足場板２Ｍ",9,6237,"FHR-15","巾木１５ (青)",3.9,6332,"SSKFBH","フックボルト（中古）"]
[72,"SS2-1ｶﾞﾀ","自在ステップ９００巾",5.5,210,"OA-2380","SKセンター主材",null,313,"FC-0914","手摺 L=９１４",2.5,null,null,null,null,1012,"A06","筋違　（白）",1.7,2008,"1.8M","丸パイプ",4.91,2112,"TB4","ターンバックル",0.6,3116,"OKSHB-606","水平筋違６０６",1.9,4023,"SPﾋﾞｰﾑ（Ｃ）","スーパービーム　中",20.52,5055,"BM1551OG","メッシュシート1524巾",4.4000000000000004,6009,"G2840","足場板４Ｍ",18,6238,"FHR-12","巾木１２ (黒)",3.3,6333,"Ｊﾌｯｸ","フラット本体取付金具",null,null,null,null,null,7647,"4.0M(N","丸パイプ日建"]
[73,"SS2-2ｶﾞﾀ","自在ステップ９００巾",9,211,"OAC-2390R","SKコーナー主材（右",null,314,"FC-1219","手摺 L=１２１９",3.2,null,null,null,null,1013,"A16S","筋違　（青）",3.5,2009,"2.0M","丸パイプ",5.46,2113,"TB5","ターンバックル",1,3117,"OKSHB-906","水平筋違９０６",2.2999999999999998,4024,"ﾋﾞｰﾑBKT","ビームブラケット水平",0,5056,"BM1851OG","メッシュシート1829巾",5.3,6010,"L1000","スカイウォーク １M",3.8,6239,"FHR-09","巾木０９ (色無)",2.8,6334,"Sｶﾅｸﾞ","巾調整用金具",null,7200,"GF1818E","ガードフェンス絵入り",17]
[74,"SS1-4ｶﾞﾀ","自在ステップ６００巾",6,212,"OAC-2390L","SKコーナー主材（左",null,315,"FC-1524","手摺 L=１５２４",3.9,null,null,null,null,1014,"A16","筋違　（茶）",3,2010,"2.5M","丸パイプ",6.83,2114,"TB6","ターンバックル",1.8,3118,"OKSHB-909","水平筋違９０９",2.6,4025,"ASBH","ブラケットサポート水平材",0,5057,"MSK","メッシュクランプ",0.4,6011,"L2000","スカイウォーク ２M",6.8,6240,"FHR-06","巾木０６ (橙)",2.2999999999999998,6335,"Lｶﾅｸﾞ","コーナー巾調整用金具Ｄ１",null,7201,"GF1812E","ミニフェンス絵入り"]
[75,"SG918","セフティアッシャー",14.8,213,"ｺｰﾅｰﾊﾟﾈﾙＡ","SKコーナーパネルA",null,316,"FC-1829","手摺 L=１８２９",4.5,null,null,null,null,1017,"A05","筋違　（桃）",2.5,2011,"3.0M","丸パイプ",8.19,2115,"ﾀｰﾝﾊﾞｯｸﾙ","ＴＢ両カン",0,3119,"OKSHB-1209","水平筋違１２０９",3,4026,"ﾊﾈﾀﾞｼﾋﾞｰﾑ-30","ハネ出しビーム３０型",17,5059,"OZS-P","親綱支柱（建枠用）",8.4,6012,"L3000","スカイウォーク ３M",10,6241,"ＦＡ３１","フック手摺１８",2.1,6336,"Jﾌｯｸ","取付金具（中古）",null,7202,"GF1818ﾄﾋﾞﾗ","ＧＦ１８１８扉"]
[76,"SS2-3ｶﾞﾀ","自在ステップ９００巾",9,214,"ｺｰﾅｰﾊﾟﾈﾙＢ","SKコーナーパネルB",null,317,null,null,null,430,"K3064S","階段枠",29,1018,"A04","筋違　（黒）",1.9,2012,"3.5M","丸パイプ",9.56,2116,"M5C","チェーン吊金具",0.85,3120,"OKSHB-1212","水平筋違１２１２",3.3,4027,"ﾊﾈﾀﾞｼﾋﾞｰﾑ-40","ハネ出しビーム４０型",19,5060,"NSP","親綱支柱（Ｈ鋼用）",8.1999999999999993,6013,"L4000","スカイウォーク ４M",13,6242,"ﾉﾋﾞｳﾏ560","のびウマ５６０",30,6337,"WS1551*","白シート（中古）",null,7203,"GF0918ﾄﾋﾞﾗ","ＧＦ０９１８扉"]
[77,"Kﾃｽﾘ12-15","階段手摺１２－１５",11.1,215,"ｺｰﾅｰﾊﾟﾈﾙＣ","SKコーナーパネルC",null,318,null,null,null,431,"K303S","階段枠Ｈ９００用",13,1019,"A03","筋違　（桃）",1.4,2013,"4.0M","丸パイプ",10.9,2119,"KS13-16","壁つなぎ130-160mm",0.72,3121,"OKSHS-15","跳ね出しステージ",17.5,4028,"ﾊﾈﾀﾞｼﾋﾞｰﾑ-60","ハネ出しビーム60型",21,5061,"ALNSP(H)","アルミ親綱支柱",6.3,6014,"ｽｷﾞｲﾀ 2M","スギイタ２Ｍ",7.5,6243,"ＦＡ３２","フック手摺１５",1.8,6338,"WS1251*","白シート（中古）",null,7204,"ｽﾁｰﾙﾍﾞｰｽ","スチールベース",9]
[78,"SU2X","階段用手摺",5.7,216,"ＯＡＣ－２３Ｃ","SKコーナーフレ止め",null,319,null,null,null,432,"K304S","階段枠Ｈ１２００用",17,1020,"A02","筋違　",0,2014,"4.5M","丸パイプ",12.3,2121,"KS18-24","壁つなぎ180-240mm",0.8,3122,"OKSBK","跳ね出しステージ金具",12,4029,"HDBL1500","跳出Ｂ水平材1.5m",6,5062,"D-POST","直交平行兼用親綱支柱",8.6999999999999993,6015,"ｽｷﾞｲﾀ 4M","杉板４M（敷板用・橙",15,6244,"ＦＡ２９","フック手摺１２",1.5,6339,"WS0951*","白シート（中古）",null,7205,"FB010","コンクリートベース"]
[79,"SS1-5ｶﾞﾀ","自在ステップ６００巾",6,217,"ＯＡＣ－２３ＥＲ","センターフレーム（右",null,320,"FK-0610","腰手摺 L=６１０",2.1,null,null,null,null,1021,"ｾﾌﾃｨｰﾌﾞﾚｽ","セフティーブレス",6,2015,"5.0M","丸パイプ",13.6,2122,"KS25-42","壁つなぎ250-420mm",1.3,3123,"OKSHSB-22","跳ね出しステージ筋違",2.4,4030,"ASBB","ブラケットサポートベース金具",0,5063,"ｼﾞｻﾞｲｶｯｼｬ","親綱緊張用自在滑車",null,6016,"ｽｷﾞｲﾀ 2M(S)","スギイタ２Ｍ(敷板)",7.5,6245,"ＦＡ２７","フック手摺０９",1.3,6340,"WS0651*","白シート（中古）",null,7206,"ﾌｪﾝｽｸﾗﾝﾌﾟ","フェンスクランプ",0.7,7802,"LT-14(NK","ラクラクタラップ１４",14]
[80,"AL4055S","アルミ階段",null,218,"ＯＡＣ－２３ＥＬ","センターフレーム（左",null,321,"FK-0914","腰手摺 L=９１４",2.4,440,"DXA-18AT","ダイナワーク 1.37m⇔1.8m",24.9,1031,"A123","アームロック",0.37,2016,"5.5M","丸パイプ",15,2123,"KS38-76","壁つなぎ380-760mm",1.5,3124,"OKSL-4*6","伸縮ブラケット",3.7,4031,"ASBK","ブラケットサポート水平材金具",0,5064,"ｶﾗﾋﾞﾅ","カラビナ",null,6017,"ｽｷﾞｲﾀ4M(S)","スギイタ４M(敷板)",15,6246,"K-1R","先行金具Ｒ (据置)",1,6341,"ﾒｶｸｼ ｱﾝｾﾞﾝ","目かくしシート",null,7207,"GFｻﾎﾟｰﾄ","フェンスサポート",1.7,7803,"LT-24(NK","ラクラクタラップ２４",21]
[81,"OS4055-06","養生枠",3,219,"ＯＡＣ－２３ＦＲ","コーナーフレーム（右",null,322,"FK-1219","腰手摺 L=１２１９",2.8,441,"DXA-15AT","ダイナワーク 1.05m⇔1.48m",22.5,1033,"A125","アームロック",0.5,2017,"6.0M","丸パイプ",16.399999999999999,2124,"KS68-106","壁つなぎ680-1060mm",2.2000000000000002,3125,"OKSL-6*8","伸縮ブラケット",4.5,4032,"ﾋﾞｰﾑW-0","ビーム金具Ｗ－０",2.8,5065,"ｱﾝｾﾞﾝｶｯｼｬ","横移動用安全滑車",null,6020,"AL4ｶﾞﾀS","アルミ脚立４尺",null,6247,"K-1L","先行金具Ｌ (据置)",1,6342,"ﾒｶｸｼ ﾑｼﾞ","目かくしシート",null,7208,"GFHｺｳｶﾅｸﾞ","フェンス用Ｈ鋼金具",1,7804,"LT-38(NK","ラクラクタラップ３８",35]
[82,"OS4055","養生枠",8,220,"ＯＡＣ－２３ＦＬ","コーナーフレーム（左",null,323,"FK-1524","腰手摺 L=１５２４",3.1,442,"DXA-10A","ダイナワーク 0.73m⇔1.07m",17,1034,"A126","アームロック",0.6,2018,"6.5M","丸パイプ",17.739999999999998,2125,"TB7","ターンバックル",0,3126,"OKSL-8*10","伸縮ブラケット",6.1,4033,"ﾋﾞｰﾑW-50","ビーム金具Ｗ－５０",3.3,5066,"ﾘﾌﾃｨﾝｸﾞP","リフティングポスト",7,6021,"3ｶﾞﾀS","脚立３尺（ステップ）",7.4,6248,"K-2R","先行金具Ｒ (先送)",1.6,6343,"WS13 ｱｽﾞｶﾘ","白シート 預り専用",null,null,null,null,null,7805,"LTT-14(NK","ラクラク手摺１４",2.5]
[83,"OS4055-09","養生枠",4,221,"OAC-UK","コーナー主材取付金具",null,324,"FK-1829","腰手摺 L=１８２９",3.5,443,"DGW-TEL","ＤＸＡ用手摺枠",4.0999999999999996,1035,"A127A","アームロック",0.41,2019,"7.0M","丸パイプ",19.11,2126,"KSﾋｶｴ","壁つなぎ控えH鋼用",1.5,3127,"ｱﾝｸﾞﾙﾊﾟﾚｯﾄ","アングルパレット",10,4034,"ﾋﾞｰﾑW-60","ビーム金具Ｗ－６０",3.4,5068,"NHG","ネットハンガー",0.63,6022,"4ｶﾞﾀS","脚立４尺（ステップ）",9.6999999999999993,6249,"K-2L","先行金具Ｌ (先送)",1.6,6344,"ﾀﾝｶﾝｷｬｯﾌﾟ","単管キャップ",null,7210,"ｶﾗｰｺｰﾝ","カラーコーン",2,7806,"LTT-24(NK","ラクラク手摺２４",3.5,9321,"WSKH","結束し"]
[84,"OS4055-12","養生枠",5.5,222,"OAC-PK","コーナー斜材取付金具",null,325,null,null,null,444,"DXA-STA18","DXA連結足場板",8.8000000000000007,1036,"A128","アームロック",0.65,2021,"8.0M","丸パイプ",21.84,null,null,null,null,3128,"ｼﾁｭｳﾊﾟﾚｯﾄ","支柱用パレット",0,4035,"HDBL2000","跳出Ｂ水平材2.0m",8,5069,"ﾛﾘｯﾌﾟ","ロリップ",0.8,6023,"6ｶﾞﾀS","脚立６尺（ステップ）",13.5,6250,"ﾍﾟｶﾞｻｽLL","ペガサス５００ＬＬ",null,null,null,null,null,7211,"ｺｰﾝﾊﾞｰ","コーンバー",1,7807]
[85,"OS48C","養生クランプ",0.5,223,"OA-3000S","コーナーセンター斜材",null,326,null,null,null,445,"DXA-AUC","DXAアウトリガー",0.9,1037,"A19A","アームロック",0.6,2024,"60K0.9M","角パイプ６０",3.65,null,null,null,null,3129,"OKARC-1","60.5×48.6(直）",0.77,4036,"NKBR-960","ブルコンロード９６０",268,5070,"Kﾛｯｸ","キョーワロック",0.63,6025,"AL4ｶﾞﾀS","アルミ脚立４尺",null,6251,"ﾌﾞﾘｯｼﾞ","ペガサス縦ブリッジ",null,null,null,null,null,7212,"ｺｰﾝｳｪｲﾄ","コーンウエイト",2,7808]
[86,"OS42C","養生クランプ",0.45,224,"OAC-09S","センター斜材用 S管",null,327,null,null,null,null,null,null,null,1038,"A124","アームロック",0.52,2025,"60K0.5M","角パイプ６０",2.0299999999999998,null,null,null,null,3130,"OKARC-2","60.5×48.6(自）",0.77,4037,"NKBR-660","ブルコンロード６６０",191,5071,"ＯＺロック","親綱緊張器",1,6026,"AL6ｶﾞﾀS","アルミ脚立６尺",null,6252,"ｻｲﾄﾞﾌﾞﾘｯｼﾞ","ペガサス横ブリッジ",null,6345,"ｺﾏｲﾀ","コマイタ",1.1000000000000001,7213,"ﾄﾗﾌｨｯｸｺｰﾝ","トラフィックコーン",3.2,7809,"LS-1010K(NK","斜面ノリダー本体",26]
[87,"OS4055-15","養生枠",6.7,225,"OAC-2980S","コーナー斜材",null,328,null,null,null,450,"SSD-6","鋼製布板メッシュ",15.2,1041,"A25(M)","手摺柱",3,2026,"60K1.0M","角パイプ６０",4.0599999999999996,null,null,null,null,3131,"OKSUJT  ","大引受ジョイント",0.5,4038,"NKSTK","Ｔ字接続金具",0,5072,"TOBI-2","トビック２型",15,6030,"ALF60","アルミ梯子６M",11.8,6253,"ﾎｼﾞｮﾃｽﾘA","ペガサス補助手摺Ａ",null,6346,"Ｍ１２ｘ９０","Ｍ１２ｘ９０ボルト",null,7214,"ｱﾙﾐﾊﾞｰ","アルミコーンバー赤白",0.7,7810,"LST-9K(NK","斜面ノリダー手摺",4,9340,"GF1818(S","ガードフェンス１８（仙台"]
[88,"OS42-C","養生４２用コーナー",0.45,226,"OAC-08S","コーナー斜材用 S管",null,329,null,null,null,451,"SSD-5","鋼製布板メッシュ",12.5,1042,"N25(O)","手摺柱（臍付）",0,2027,"60K1.5M","角パイプ６０",6.09,null,null,null,null,3132,"OKSH-3","水平ブレス３０５Ｌ",1.3,4039,"NKK800","カサアゲ金具",24.4,5073,"Gﾛｰﾌﾟ","ガードロープ",1.4,6031,"ALF30","アルミ梯子３M",5.9,6254,"ﾎｼﾞｮﾃｽﾘB","ペガサス補助手摺Ｂ",null,6347,"Ｍ１２ﾅｯﾄ","Ｍ１２ナット",null,7215,"ｱｵｼﾛｺｰﾝ","青白コーン",3.2,null,null,null,null,9341,"ﾌｪﾝｽﾍﾞｰｽ(S","ベース（仙台"]
[89,"OSK","養生兼用クランプ",0.45,227,"OA-2306A15","SKバンノー受L15",null,330,"FL-0610","斜材　６／８６",1.9,452,"SSD-4","鋼製布板メッシュ",10.5,1046,"A26","手摺",0.7,2028,"60K2.0M","角パイプ６０",8.1199999999999992,null,null,null,null,3133,"OKC-1","ＯＫクランプ直交",1.7,4040,"NKKK","固定金具",0.8,5081,"ｽｶｲｽﾃｯﾌﾟ10ｶﾞﾀ","スカイステップ１０型",21,6032,"ALF60S","アルミ２連梯子６M",12.3,6255,"CSR-100D","マイティー１００型",11.1,6348,"ｸﾘｱｼｰﾄ15","クリアシート１５",3.4,7216,"ｱｵｼﾛﾊﾞｰ","アルミコーンバー青白",0.7,7854,"ﾊﾟﾈﾙｹﾞｰﾄ63（ｓ）","パネルゲートPGN63",520,9342,"　　Fｸﾗﾝﾌﾟ（S","ﾌｪﾝｽｸﾗﾝﾌﾟ（仙台"]
[90,"OSK-C","養生兼用コーナー",0.45,228,"OA-2306D15","SKバンノー受C15",null,331,"FL-0914","斜材　９／１７",3.1,455,"SSD-624","鋼製布板メッシュ",9.9,1047,"A27","手摺914",0.9,2029,"60K2.5M","角パイプ６０",10.199999999999999,null,null,null,null,3134,"OKC-2","ＯＫクランプ自在",1.6,4041,"NKBR","ブルコンロード用手摺",null,null,null,null,null,6033,"ALF40","アルミ梯子４M",7.2,6256,"ﾉﾋﾞｳﾏﾃｽﾘ","のびうま手摺",2.4,6349,"ｸﾘｱｼｰﾄ12","クリアシート１２",2.8,7217,"ﾐﾄﾞﾘｼﾛｺｰﾝ","緑白コーン",3.2,null,null,null,null,9343,"ｶﾗｰｺｰﾝ（S","カラーコーン（仙台"]
[91,"A143","梁枠２スパン",33.1,229,"OA-2306B15","SKバンノー押え15",null,332,"FL-1219","斜材　１２／１７",3.2,456,"SSD-524","鋼製布板メッシュ",8.5,1048,"A28","手摺610",0.5,2030,"60K3.0M","角パイプ６０",12.2,3001,"90ｶﾞﾀ","サポート９尺2616-3948mm",14.5,3135,"OKSS-3","ＯＫ支柱３２４",2.2999999999999998,4042,"ﾂﾘｱｼﾊﾞ1500","吊足場",11,5100,"SGNT","階段開口ネットたて型",0.7,6034,"ALF66S","アルミハシゴ（二連）",12.3,6257,"FA28","フック手摺０６",1,6350,"ｸﾘｱｼｰﾄ09","クリアシート０９",2.2000000000000002,7218,"ﾐﾄﾞﾘｼﾛﾊﾞｰ","アルミコーンバー緑白",0.7,null,null,null,null,9344,"ｺｰﾝﾊﾞｰ（S","コーンバー（仙台"]
[92,"A147","梁枠３スパンL=6700",45.3,230,"OA-2306C15","SKフレ止め15",null,333,"FL-1524","斜材　１５／１７",3.5,457,"SSD-424","鋼製布板メッシュ",7,1049,"A29","手摺1219",1.2,2031,"60K3.5M","角パイプ６０",14.2,3003,"70ｶﾞﾀ","サポート７尺2116-3448mm",13,3136,"OKS-A752PJ","ＯＫピポットジャッキ",4.7,4043,"ﾂﾘｱｼﾊﾞ1700","吊足場",11.7,5101,"SGNY","階段開口ネットよこ型",0.5,6035,"ALF93S","アルミハシゴ（二連）",22.8,null,null,null,null,6351,"ｸﾘｱｼｰﾄ06","クリアシート０６",1.6,7220,"ﾌﾟﾗｶﾞｰﾄﾞ","プラガード",2.2999999999999998,8150,"AX11-14","ＡＸビーム",11.3,9345,"ﾌﾟﾗｶﾞｰﾄﾞ(S","プラガード（仙台"]
[93,"A148","梁枠",33.1,231,"OA-2306A12","SKバンノー受L12",null,334,"FL-1829","斜材　１８／１７",3.7,null,null,null,null,1050,"A31","手摺1829",1.7,2032,"60K4.0M","角パイプ６０",16.2,null,null,null,null,3137,"OKSIS-9","移動用支持材",5,4044,"ｶﾀﾂﾘｱｼﾊﾞ","吊足場片面",7.6,null,null,null,null,6036,"NKB300M","伸縮ブラケット230-340mm",3.2,null,null,null,null,6352,"ｼﾞｬｯｷｿｯｸｽ","ジャッキソックス",0,7221,"ﾌﾟﾗｶﾞｰﾄﾞK","プラガード角型",null,8151,"AX14-18","ＡＸビーム",12.5]
[94,"A149","梁枠４スパンL=8000",58,232,"OA-2306D12","SKバンノー受C12",null,335,null,null,null,460,"TOBI-4","トビック４型",19,1051,"A32","手摺1524",1.5,2033,"60K4.5M","角パイプ６０",18.3,3005,"60ｶﾞﾀ","サポート６尺1716-3048mm",12,3138,"OKSISJ-125","移動用ジャッキ車輪",10.5,4046,"L9-20","セーブマン",2,null,null,null,null,6037,"NKB500","伸縮ブラケット330-500mm",4.2,6260,"RK305S","ローリング用内階段",null,6353,"Kｼｰﾄ4M","開口シート４ｍ",2,7222,"BS010","スタンドバリケード",null,8152,"AX18-25","ＡＸビーム",19]
[95,"A147(M)","梁枠３スパンL=6000",37.700000000000003,233,"OA-2306B12","SKバンノー押え12",null,336,null,null,null,null,null,null,null,null,null,null,null,2034,"60K5.0M","角パイプ６０",20.3,3008,"40ｶﾞﾀ","サポート４尺1216-2003mm",9.5,3139,"OKSPH","大引受金具",2.2000000000000002,4047,"L9-30","セーブマン",2,null,null,null,null,6038,"NKB750","伸縮ブラケット500-750mm",5.4,6261,"RAL305S","内階段（アルミ）",null,6354,"Kｼｰﾄ1.4M","開口シート１．４ｍ",1,7223,"オモシ","単管用オモシ",8,8153,"AX25-32","ＡＸビーム",23]
[96,"A150","梁渡（１２１９用）",10.199999999999999,234,"OA-2306C12","SKフレ止め12",null,337,null,null,null,470,"PNF-18L","スカイフェンス18",8.8000000000000007,1053,"CG6-12ｺﾉｼﾞ","妻手摺コの字型",2.5,2035,"60K5.5M","角パイプ６０",22.3,3009,"30ｶﾞﾀ","サポート３尺916-1423mm",7.5,3140,"OKSKJ-4030","ＯＫ壁当てジャッキ",2.5,4048,"L1500SL","伸縮片吊足場",11,null,null,null,null,6039,"NKB1000","伸縮ブラケット750-1000mm",6.4,6262,"HTR6","ローリング用ハッチ",null,6355,"Pｸﾘｯﾌﾟ","パッチンクリップ",null,7225,"Ｆホルダー","工事灯金具",0.12,8154,"AX32-39","ＡＸビーム",28]